band_pass               Band-pass signals
baseline_array          Calculate Contrasts of Arrays in Different
                        Methods
butter_max_order        'Butterworth' filter with maximum order
check_filter            Check 'Arma' filter
collapse                Collapse array
convolve                Convolution of '1D', '2D', '3D' data via 'FFT'
decimate                Decimate with 'FIR' or 'IIR' filter
design_filter           Design a digital filter
design_filter_fir       Design "FIR" filter using 'firls'
design_filter_iir       Design an 'IIR' filter
detrend                 Remove the trend for one or more signals
diagnose_channel        Show channel signals with diagnostic plots
diagnose_filter         Diagnose digital filter
dijkstras-path          Calculate distances along a surface
fast_cov                Calculate massive covariance matrix in parallel
fast_quantile           Compute quantiles
fill_surface            Fill a volume cube based on water-tight surface
filter-window           Filter window functions
filter_signal           Filter one-dimensional signal
filtfilt                Forward and reverse filter a one-dimensional
                        signal
find_peaks              Find peaks of a signal
fir1                    Window-based 'FIR' filter design
firls                   Least-squares linear-phase 'FIR' filter design
freqz2                  Frequency response of digital filter
gammatone_fast          Apply gamma-tone filters to obtain auditory
                        envelopes
grow_volume             Grow volume mask
internal_rave_function
                        Get external function from 'RAVE'
left_hippocampus_mask   Left 'Hippocampus' of 'N27-Collin' brain
matlab_palette          'Matlab' heat-map plot palette
mesh_from_volume        Generate 3D mesh surface from volume data
multitaper              Compute 'multitaper' spectral densities of
                        time-series data
naive_nmf               A naive implementation of non-negative matrix
                        factorization
new_matrix4             Create a 'Matrix4' instance for "Affine"
                        transform
new_quaternion          Create a 'Quaternion' instance to store '3D'
                        rotation
new_vector3             Create a 'Vector3' instance to store '3D'
                        points
notch_filter            Apply 'Notch' filter
parallel-options        Set or get thread options
plane_geometry          Create a two-dimensional plane in three
                        dimensional space
plot_signals            Plot one or more signal traces in the same
                        figure
project_plane           Project plane to a surface
pwelch                  Calculate 'Welch Periodogram'
raw-to-sexp             Convert raw vectors to R vectors
rcond_filter_ar         Computer reciprocal condition number of an
                        'Arma' filter
register_volume         Imaging registration using "NiftyReg"
resample_3d_volume      Sample '3D' volume in the world (anatomical
                        "RAS") space
rgl-call                Safe ways to call package "rgl" without
                        requiring "x11"
shift_array             Shift array by index
stimpulse_interpolate   Find and interpolate stimulation pulses
stimulation_signal      Sample stimulation recording
vcg_isosurface          Create surface mesh from 3D-array
vcg_kdtree_nearest      Find nearest 'k' points
vcg_mesh_volume         Compute volume for manifold meshes
vcg_raycaster           Cast rays to intersect with mesh
vcg_smooth              Implicitly smooth a triangular mesh
vcg_sphere              Simple 3-dimensional sphere mesh
vcg_subdivision         Sub-divide (up-sample) a triangular mesh
vcg_subset_vertex       Subset mesh by vertex
vcg_uniform_remesh      Sample a surface mesh uniformly
vcg_update_normals      Update vertex normal
wavelet                 'Morlet' wavelet transform (Discrete)
